# Instalação de Patch via CLI

Last modified by Jean Franco on 2022/06/28 14:27
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Tempo estimado

No. | Operation Item | Estimated Time (Unit: Minute)
1 | Check the device status. | 3
2 | Save and back up the data. | 5
3 | Load the patch. | 30
4 | Activate and run the patch. | 20
5 | Verify the patch installation. | 1

Preparando para a Instalar

1. Verificando a versão do sistema

MA5800-X7(config)#display language

{ <cr>||<K> }:

Command:

display language

Local:

Description: CHINESE SIMPLIFIED (DEFAULT LANGUAGE)

Version: MA5800V100R018C00

Encoding: GBK

General:

Description: ENGLISH (DEFAULT LANGUAGE)

Version: MA5800V100R018C00

Encoding: ANSI

MA5800-X7(config)#display patch all

{ <cr>||<K> }:

Command:

display patch all

Software Version:MA5800V100R018C00

SPH105

HP1010; HP1020

HP1102

------------------------------------------------------------------------

Current Patch State:

------------------------------------------------------------------------

Patch Name Patch State Delivery Attribute Dependency

------------------------------------------------------------------------

SPH105 running common hot patch NO

HP1010 running common hot patch NO

HP1020 running common hot patch YES

HP1102 running common hot patch NO

------------------------------------------------------------------------

Total:4

Patches in the system cannot be rolled back

2. Checar o estado do equipamento

MA5800-X2>display board 0

{ <cr>||<K> }:

Command:

display board 0

-------------------------------------------------------------------------

SlotID BoardName Status SubType0 SubType1 Online/Offline

-------------------------------------------------------------------------

0 H901PISA Normal

1 H902GPSF Normal

2

3 H901MPSA Standby_failed CPCA Offline

4 H901MPSA Active_normal CPCA

5

-------------------------------------------------------------------------

3. Backup do banco de dados:

MA5800-X7(config)#backup data sftp 10.11.104.1 sysdata.dat

Please save database file before backup, or the database file that is backed

up may not be the latest one. Are you sure to continue? (y/n)[n]: y

MA5800-X7(config)#backup configuration sftp 10.11.104.1 config.txt

Please save configuration file before backup, or the configuration file that

is backed up may not be the latest. Are you sure to continue? (y/n)[n]:y

----End

4. Instalando o arquivo de Patch:

1. Load, activate and run the Patch file V100R018C00SPH109_wholepatch_MPLB_TDC.

MA5800-X7(config)#load patch sftp 10.11.104.1 V100R018C00SPH109_wholepatch_MPLB_TDC

MA5800-X7(config)#patch activate SPH109

MA5800-X7(config)#patch run SPH109

5. Verificando:

Run the following commands to check whether the patch is installed correctly.

MA5800-X7(config)#display patch all

{ <cr>||<K> }:

Command:

display patch all

Software Version:MA5800V100R018C00

SPH109

HP1010

------------------------------------------------------------------------

Current Patch State:

------------------------------------------------------------------------

Patch Name Patch State Delivery Attribute Dependency

------------------------------------------------------------------------

SPH109 running common hot patch NO

HP1010 running common hot patch NO

------------------------------------------------------------------------

Total:2

Last Patch State:

------------------------------------------------------------------------

Patch Name Patch State Delivery Attribute Dependency

------------------------------------------------------------------------

SPH105 running common hot patch NO

HP1010 running common hot patch NO

HP1020 running common hot patch YES

------------------------------------------------------------------------

6. Voltando um Patch:

Procedimento:

1. Obtenha o pacote combinado da versão fonte, e coloque no servidor de TFTP.

2. Obtenha o banco de dados que foi feito o backup antes do procedimento de backup, e coloque no servidor de TFTP.

CUIDADO: Você precisa usar o banco de dados da versão que foi feito o backup antes de atualizar, caso contrário a config pode não funcionar.

3. Carregue o arquivo combinado.

Execute:

load packetfile

Execute: display progress load para visualizar o andamento do carregamento.

Execute: load data para carregar o backup do banco de dados.

Execute: upgrade para resetar o sistema.

Exemplo:

- The SFTP file transfer mode is used.
- The IP address of the file transfer server is x.x.x.x.
- The combined package file is

V100R018C00HP1102_wholepackage(SPC100)_MPLB_for_TDC.bin.

- The database file that is backed up before the upgrade is sysdata.dat.

MA5800-X7(config)#load packetfile sftp x.x.x.x V100R018C00HP1102_wholepackage(SPC100)_MPLB_for_TDC.bin
The new packet file will overwrite the old one

Rollback function will be disabled

Be sure that the system needn't this function

Are you sure to load new packet file? (y/n)[n]:y

MA5800-X7(config)#load data sftp x.x.x.x sysdata.dat all
The new database will overwrite the old one
Rollback function will be disabled
Be sure that the system needn't this function
It's irreversible. Are you sure to load new database? (y/n)[n]:y

MA5800-X7(config)#upgrade
{ <cr>|emergency-call-protect<K>|issu<K>|mpls<K> }:

Command:

upgrade

Software upgrades will lead to business interruption, continue? (y/n)[n]:y

0
Tags:
Created by Jean Franco on 2022/06/28 14:15

- Comments (0)
- Attachments (0)
- History
- Information

# Applications

# Tips

Did you know that you can improve XWiki? Take 5 minutes to fill this survey and help this open source project!

Maila Networks
XWiki Debian 14.4.1