Ubiquiti - BGP peering with an ISP 

Page / - last modified by Jean Franco on 2024/06/09 22:16 

BGP peering with an ISP 
last modified by Jean Franco
on 2024/06/09 22:16

Table of Contents
Overview
The Prefix Lists
The Route Maps
BGP Protocol Configuration
Showing BGP Information

Overview
When you have your own IPv4/IPv6 address space, it's advantageous to announce it via your router to your ISP - especially if you have multiple providers (multi-homing). Even the lowest end EdgeRouters such as the ER-X and ERL can do a full BGP table.
The Prefix Lists
The prefix lists are used to control what routes you get from your ISP, as well as the ones you send (announce).
policy { prefix-list BGP-ISP-From { rule 10 { action permit le 24 prefix 0.0.0.0/0 } } prefix-list BGP-ISP-To { rule 10 { action permit prefix 192.0.2.0/24 } } prefix-list6 BGP-ISPv6-From { rule 10 { action permit le 64 prefix 0::/0 } } prefix-list6 BGP-ISPv6-To { rule 10 { action permit le 48 prefix 2001:DB8::/32 } } }
The -From prefix lists are for routes you receive (imported) from your ISP, while the -To lists are for routes being exported (announced) to your provider. In the case of IPv4, the smallest globally accepted size most if not all providers announce is /24. For IPv6, the smallest globally accepted size is /48.
'le' means any prefix smaller (ie: 'le 48' won't allow a /64 IPv6 prefix from your ISP's routing table, but it will allow a /32). 'ge' means any prefix greater (ie: 'ge 56' won't allow a /48, but will allow a /56, /64, or even /128).
In the above examples, 192.0.2.0/24 is your IPv4 netblock, and 2001:DB8::/32 is your IPv6 one. 0.0.0.0/0 and 0::/0 means match all.
The Route Maps
While you can just use prefix lists with BGP to control routes imported and exported, route maps give you much more flexibility and control, and can even include AS path matching.
policy { route-map BGP-ISPv6-From { rule 10 { action permit match { ipv6 { address { prefix-list BGP-ISPv6-From } } } } } route-map BGP-ISPv6-To { rule 10 { action permit match { ipv6 { address { prefix-list BGP-ISPv6-To } } } } } route-map BGP-ISP-From { rule 10 { action permit match { ip { address { prefix-list BGP-ISP-From } } } } } route-map BGP-ISP-To { rule 10 { action permit match { ip { address { prefix-list BGP-ISP-To } } } } } }
Like the prefix lists, -To and -From are your specific directions in and out (import and export). They're pretty self explanatory and reference the prefix lists used before.
BGP Protocol Configuration
protocols { bgp 65501 { address-family { ipv6-unicast { network 2001:DB8::/32 { } } } neighbor 100.64.100.1 { remote-as 65502 route-map { export BGP-ISP-To import BGP-ISP-From } soft-reconfiguration { inbound } update-source 100.64.100.2 } neighbor fd00::1 { address-family { ipv6-unicast { route-map { export BGP-ISPv6-To import BGP-ISPv6-From } } } remote-as 65502 soft-reconfiguration { inbound } update-source fd00::2 } network 192.0.2.0/24 { } parameters { router-id 100.64.100.2 } redistribute { connected { } kernel { } static { } } } }
In the above example, our local router has the IPv4 address of 100.64.100.2 and the IPv6 address of fd00::2 with an ASN of 65501. The BGP enabled router on our ISP side is 100.64.100.1 and fd00::1 with an ASN of 65502. We are assuming that our routers are connected over a non-shared link within one hop. If the BGP router is more than one hop away, you need to configure 'ebgp-multihop' with the appropriate amount of hops away your ISP's router is.
Showing BGP Information
user@router1:~$ show ip bgp neighbor
BGP neighbor is 100.64.100.2, remote AS 65502, local AS 65501, external link
  BGP version 4, remote router ID 100.64.100.2
  BGP state = Established, up for 01w0d05h
  Last read 01w0d05h, hold time is 90, keepalive interval is 30 seconds
  Neighbor capabilities:
    Route refresh: advertised and received (old and new)
    4-Octet ASN Capability: advertised and received
    Address family IPv4 Unicast: advertised and received
    Address family IPv4 Multicast: received
  Received 2838376 messages, 0 notifications, 0 in queue
  Sent 20788 messages, 0 notifications, 0 in queue
  Route refresh request: received 0, sent 0
  Minimum time between advertisement runs is 30 seconds
  Update source is 100.64.100.1
 For address family: IPv4 Unicast
  BGP table version 6603726, neighbor version 6603716
  Index 2, Offset 0, Mask 0x4
  Inbound soft reconfiguration allowed
  Community attribute sent to this neighbor (both)
  Inbound path policy configured
  Outbound path policy configured
  Route map for incoming advertisements is *BGP-ISP-From
  Route map for outgoing advertisements is *BGP-ISP-To
  688930 accepted prefixes
  1 announced prefixes

 Connections established 1; dropped 0
  External BGP neighbor may be up to 1 hops away.
Local host: 100.64.100.2, Local port: 60803
Foreign host: 100.64.100.1, Foreign port: 179
Nexthop: 100.64.100.1
BGP connection: shared network

BGP neighbor is fd00::1, remote AS 65502, local AS 65501, external link
  BGP version 4, remote router ID 100.64.100.1
  BGP state = Established, up for 01w0d05h
  Last read 01w0d05h, hold time is 180, keepalive interval is 60 seconds
  Neighbor capabilities:
    Route refresh: advertised and received (old and new)
    4-Octet ASN Capability: advertised and received
    Address family IPv4 Unicast: advertised
    Address family IPv6 Unicast: advertised and received
  Received 686685 messages, 0 notifications, 0 in queue
  Sent 10394 messages, 0 notifications, 0 in queue
  Route refresh request: received 0, sent 0
  Minimum time between advertisement runs is 30 seconds
  Update source is fd00::2
 For address family: IPv4 Unicast
  BGP table version 6603726, neighbor version 6603716
  Index 1, Offset 0, Mask 0x2
  Inbound soft reconfiguration allowed
  Community attribute sent to this neighbor (both)
  0 accepted prefixes
  0 announced prefixes

 For address family: IPv6 Unicast
  BGP table version 858622, neighbor version 858620
  Index 1, Offset 0, Mask 0x2
  Community attribute sent to this neighbor (both)
  Inbound path policy configured
  Outbound path policy configured
  Route map for incoming advertisements is *BGP-ISPv6-From
  Route map for outgoing advertisements is *BGP-ISPv6-To
  49892 accepted prefixes
  1 announced prefixes

 Connections established 1; dropped 0
Local host: fd00::2, Local port: 179
Foreign host: fd00::1, Foreign port: 8044
Nexthop: 100.64.100.1
Nexthop global: fd00::1
BGP connection: shared network