# Exemplo de BGP config

Last modified by Jean Franco on 2024/06/09 20:43
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

username@dr-ER4-BGP-RTR1:~$ show configuration

firewall {

group {

network-group ALLOWED_ADMIN_GROUP {

network 38.x.x.0/24

network 38.x.x.128/26

network 38.x.x.0/24

network 10.x.x.0/24

network 10.x.x.0/24

network 172.x.x.0/24

network 10.x.x.0/24

network 10.x.x.0/24

}

}

name REMOTE_ACCESS {

default-action drop

description "IPv4 inbound traffic to the router"

enable-default-log

rule 5 {

action accept

description "Allow Established"

log disable

protocol all

state {

: established enable

related enable

}

}

rule 10 {

action accept

description "Allow BGP"

destination {

port 179

}

log disable

protocol tcp

}

rule 20 {

action accept

description "Allow ICMP"

log disable

protocol icmp

}

rule 30 {

action accept

description "Allow SNMP"

destination {

: port 161

}

log disable

protocol udp

source {

group {

network-group ALLOWED_ADMIN_GROUP

}

}

}

rule 40 {

action accept

description "Allow SSH"

destination {

port 22

}

log disable

protocol tcp

source {

group {

network-group ALLOWED_ADMIN_GROUP

}

}

: }

rule 50 {

action accept

description "Allow HTTPS"

destination {

port 443

}

log disable

protocol tcp

source {

group {

network-group ALLOWED_ADMIN_GROUP

}

}

}

rule 60 {

action accept

description "Allow HTTP"

destination {

port 80

}

log disable

protocol tcp

: source {

group {

network-group ALLOWED_ADMIN_GROUP

}

}

}

}

}

interfaces {

ethernet eth0 {

address 38.x.x.1/24

description "USABLE BGP CLASS C FROM COGENT"

duplex auto

firewall {

local {

name REMOTE_ACCESS

}

}

speed auto

}

ethernet eth1 {

address 144.x.x.230/30

description "LIGHTTOWER 200"

: duplex auto

firewall {

local {

name REMOTE_ACCESS

}

}

speed auto

}

ethernet eth2 {

duplex auto

firewall {

local {

name REMOTE_ACCESS

}

}

speed auto

}

ethernet eth3 {

address 38.x.x.126/30

description "COGENT 1000"

duplex full

firewall {

local {

: name REMOTE_ACCESS

}

}

speed 1000

}

}

policy {

prefix-list BGP {

}

prefix-list EXPORT {

rule 10 {

action permit

prefix 38.x.x.0/24

}

}

prefix-list IMPORT {

rule 20 {

action permit

prefix 0.0.0.0/0

}

}

}

protocols {

: bgp 5xxx1 {

neighbor 38.x.x.125 {

description "COGENT AS Neighbor"

prefix-list {

export EXPORT

import IMPORT

}

remote-as 174

soft-reconfiguration {

inbound

}

}

neighbor 144.x.x.229 {

description "LIGHTOWER AS Neighbor"

prefix-list {

export EXPORT

import IMPORT

}

remote-as 46887

soft-reconfiguration {

inbound

}

}

: network 38.x.x.0/24 {

}

}

static {

route 38.x.x.0/24 {

blackhole {

}

}

}

}

service {

gui {

http-port 80

https-port 443

older-ciphers enable

}

snmp {

community XXX_SNMP_RO {

authorization ro

}

}

ssh {

port 22

: protocol-version v2

}

ubnt-discover {

disable

}

unms {

disable

}

}

system {

host-name dr-ER4-BGP-RTR1

login {

user username {

authentication {

encrypted-password ****************

plaintext-password ****************

}

full-name ""

level admin

}

user ubnt {

authentication {

encrypted-password ****************

: }

level admin

}

}

name-server 8.8.8.8

ntp {

server 0.ubnt.pool.ntp.org {

}

server 1.ubnt.pool.ntp.org {

}

server 2.ubnt.pool.ntp.org {

}

server 3.ubnt.pool.ntp.org {

}

}

syslog {

global {

facility all {

level notice

}

facility protocols {

level debug

}

: }

}

time-zone America/New_York

}

0
Tags:
Created by Jean Franco on 2024/06/09 20:41

- Comments (1)
- Attachments (0)
- History
- Information

# Applications

# Tips

When editing in WYSIWYG, type [ and then start typing letters to get suggestions for creating a link.

Maila Networks
XWiki Debian 14.4.1