# Wiki source code of FreeRADIUS EAP-TLS Example for 1x Authentication

Last modified by Jean Franco on 2022/06/23 22:09
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Show last authors

author | version | line-number | content
--- | --- | --- | ---
|  | 1 | == Create Necessary Certificates ==
|  | 2 |
|  | 3 | Follow guide [[here>>url:http://deployingradius.com/]] for creating certificates.
|  | 4 |
|  | 5 | You'll need to put the ca.pem, dh, server.key, and server.pem files in /etc/freeradius/certs.
|  | 6 |
|  | 7 | == Set up eap.conf ==
|  | 8 |
|  | 9 | Below is an example of what you need to put in /etc/freeradius/eap.conf to handle the proper authentication methods, as well as enable future functionality.
|  | 10 |
|  | 11 | {{code language="none"}}
|  | 12 | # -*- text -*-
|  | 13 | ##
|  | 14 | ## eap.conf -- Configuration for EAP types (PEAP, TTLS, etc.)
|  | 15 | ##
|  | 16 |
|  | 17 | eap {
|  | 18 | default_eap_type = md5
|  | 19 | timer_expire = 60
|  | 20 | ignore_unknown_eap_types = no
|  | 21 | cisco_accounting_username_bug = no
|  | 22 | max_sessions = ${max_requests}
|  | 23 |
|  | 24 | md5 {
|  | 25 | }
|  | 26 |
|  | 27 | leap {
|  | 28 | }
|  | 29 |
|  | 30 | gtc {
|  | 31 | #challenge = "Password: "
|  | 32 | auth_type = PAP
|  | 33 | }
|  | 34 |
|  | 35 | tls {
|  | 36 | certdir = ${confdir}/certs
|  | 37 | cadir = ${confdir}/certs
|  | 38 | private_key_password = whatever
|  | 39 | private_key_file = ${certdir}/server.key
|  | 40 | certificate_file = ${certdir}/server.pem
|  | 41 | CA_file = ${cadir}/ca.pem
|  | 42 | dh_file = ${certdir}/dh
|  | 43 | random_file = /dev/urandom
|  | 44 | #fragment_size = 1024
|  | 45 | #include_length = yes
|  | 46 | #check_crl = yes
|  | 47 | CA_path = ${cadir}
|  | 48 | #check_cert_issuer = "/C=GB/ST=Berkshire/L=Newbury/O=My Company Ltd"
|  | 49 | #check_cert_cn = %{User-Name}
|  | 50 | cipher_list = "DEFAULT"
|  | 51 | #virtual_server = check-eap-tls
|  | 52 | make_cert_command = "${certdir}/bootstrap"
|  | 53 | ecdh_curve = "prime256v1"
|  | 54 | cache {
|  | 55 | enable = no
|  | 56 | lifetime = 24 # hours
|  | 57 | max_entries = 255
|  | 58 | }
|  | 59 |
|  | 60 | verify {
|  | 61 | #tmpdir = /tmp/radiusd
|  | 62 | #client = "/path/to/openssl verify -CApath ${..CA_path} %{TLS-Client-Cert-Filename}"
|  | 63 | }
|  | 64 | ocsp {
|  | 65 | enable = no
|  | 66 | override_cert_url = yes
|  | 67 | url = "http://127.0.0.1/ocsp/"
|  | 68 | # use_nonce = yes
|  | 69 | # timeout = 0
|  | 70 | # softfail = no
|  | 71 | }
|  | 72 | }
|  | 73 |
|  | 74 | ttls {
|  | 75 | default_eap_type = md5
|  | 76 | copy_request_to_tunnel = no
|  | 77 | use_tunneled_reply = yes
|  | 78 | virtual_server = "inner-tunnel"
|  | 79 | #include_length = yes
|  | 80 | }
|  | 81 | peap {
|  | 82 | default_eap_type = mschapv2
|  | 83 | copy_request_to_tunnel = no
|  | 84 | use_tunneled_reply = yes
|  | 85 | #proxy_tunneled_request_as_eap = yes
|  | 86 | virtual_server = "inner-tunnel"
|  | 87 | #soh = yes
|  | 88 | #soh_virtual_server = "soh-server"
|  | 89 | }
|  | 90 |
|  | 91 | mschapv2 {
|  | 92 | #send_error = no
|  | 93 | }
|  | 94 | }
|  | 95 | {{/code}}
|  | 96 |
|  | 97 | == Set up clients.conf ==
|  | 98 |
|  | 99 | You'll need a client configuration for each Unifi device (or device group) that will be querying the FreeRADIUS server.
|  | 100 |
|  | 101 | **Note:** //each device (such as a UAP) will need to have to connectivity to the FreeRADIUS server - this includes both a network route, and TCP/UDP ports 1812 and 1813.//
|  | 102 |
|  | 103 | In /etc/freeradius/clients.conf, add one group like:
|  | 104 |
|  | 105 | {{code language="none"}}
|  | 106 | client 192.168.0.0/24 {
|  | 107 | secret = CHANGEME
|  | 108 | nastype = other
|  | 109 | }
|  | 110 | {{/code}}
|  | 111 |
|  | 112 | You can use single IPs (192.168.0.2 or 2001::beef) or netblocks (192.168.0.0/24 or 2001:beef::/64), and the device with that single IP or devices within that netblock will use the password specified as 'CHANGEME'.
|  | 113 |
|  | 114 | == Set up the users file ==
|  | 115 |
|  | 116 | Users can be manually set up with entries in /etc/freeradius/users.
|  | 117 |
|  | 118 | A basic user example is:
|  | 119 |
|  | 120 | {{{
|  | 121 | joeuser Cleartext-Password := "passwordhere"}}}
|  | 122 |
|  | 123 | A more complex one that also involves setting a VLAN that a user is part of:
|  | 124 |
|  | 125 | {{{joeuser Cleartext-Password := "passwordhere"
|  | 126 | Tunnel-Type = 13,
|  | 127 | Tunnel-Medium-Type = 6,
|  | 128 | Tunnel-Private-Group-Id = 2}}}
|  | 129 |
|  | 130 | Tunnel-Private-Group-Id is set to the VLAN ID you wish the user to be assigned when they connect.

# Applications

# Tips

You can click on the arrows next to the breadcrumb elements to quickly navigate to sibling and children pages.

Maila Networks
XWiki Debian 14.4.1