Ubiquiti - IPSec 

Page / - last modified by Jean Franco on 2022/07/18 21:41 

IPSec 
last modified by Jean Franco
on 2022/07/18 21:41

Table of Contents

Exemplo de config de IPSec StrongSwan:
ubnt@ubnt# show vpn ipsec
 allow-access-to-local-interface disable
 auto-firewall-nat-exclude enable
 esp-group FOO1 {
     compression disable
     lifetime 43200
     mode tunnel
     pfs dh-group20
     proposal 1 {
         encryption aes256
         hash sha256
     }
 }
 ike-group FOO1 {
     ikev2-reauth no
     key-exchange ikev2
     lifetime 7200
     proposal 1 {
         dh-group 20
         encryption aes256
         hash sha256
     }
 }
 nat-traversal enable
 site-to-site {
     peer 62.X.X.X {
         authentication {
             id 178.X.X.X
             mode pre-shared-secret
             pre-shared-secret SECRET
         }
         connection-type initiate
         description R
         ike-group FOO1
         ikev2-reauth inherit
         local-address any
         tunnel 1 {
             allow-nat-networks disable
             allow-public-networks enable
             esp-group FOO1
             local {
                 prefix 192.168.178.0/24
             }
             remote {
                 prefix 10.99.10.67/32
             }
         }
     }
 }