# Wiki source code of TFTP to Cisco Phones

Last modified by Jean Franco on 2022/06/23 22:09
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Show last authors

author | version | line-number | content
--- | --- | --- | ---
|  | 1 | = TFTP Server To Cisco VoIP Phones =
|  | 2 |
|  | 3 | Cisco 7900 series phones will want a TFTP server via DHCP options on boot in order to configure themselves.
|  | 4 |
|  | 5 | {{{ set service dhcp-server global-parameters 'option tftp66 code 66 = ip-address;'
|  | 6 | set service dhcp-server global-parameters 'option tftp150 code 150 = ip-address;'}}}
|  | 7 |
|  | 8 | {{{ set service dhcp-server shared-network-name VoIP subnet 192.168.0.0/24 subnet-parameters 'option tftp66 192.168.0.253;'
|  | 9 | set service dhcp-server shared-network-name VoIP subnet 192.168.0.0/24 subnet-parameters 'option tftp150 192.168.0.253;'}}}
|  | 10 |
|  | 11 | While we're at it, lets also tell new Unifi devices where to pick up the controller!
|  | 12 |
|  | 13 | {{{ set service dhcp-server shared-network-name LAN subnet 192.168.0.0/24 unifi-controller 192.168.0.253}}}

# Applications

# Tips

Jump to any page in the wiki with Ctrl+G or Meta+G.
See more shortcuts.

Maila Networks
XWiki Debian 14.4.1