# TFTP to Cisco Phones

Last modified by Jean Franco on 2022/06/23 22:09
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

# TFTP Server To Cisco VoIP Phones

Cisco 7900 series phones will want a TFTP server via DHCP options on boot in order to configure themselves.

      set service dhcp-server global-parameters 'option tftp66 code 66 = ip-address;'
      set service dhcp-server global-parameters 'option tftp150 code 150 = ip-address;'

      set service dhcp-server shared-network-name VoIP subnet 192.168.0.0/24 subnet-parameters 'option tftp66 192.168.0.253;'
      set service dhcp-server shared-network-name VoIP subnet 192.168.0.0/24 subnet-parameters 'option tftp150 192.168.0.253;'

While we're at it, lets also tell new Unifi devices where to pick up the controller!

      set service dhcp-server shared-network-name LAN subnet 192.168.0.0/24 unifi-controller 192.168.0.253

0
Tags:
Created by Jean Franco on 2022/06/23 22:09

- Comments (0)
- Attachments (0)
- History
- Information

# Applications

# Tips

When editing in WYSIWYG, type [ and then start typing letters to get suggestions for creating a link.

Maila Networks
XWiki Debian 14.4.1