# Comissionamento

Last modified by Jean Franco on 2024/06/10 17:56
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Criando usuários:

username zte password zte max-sessions 1 privilege 15

username usuario01 password Usuario@123 max-sessions 1 privilege 15

username usuario02 password Usuario@123 max-sessions 1 privilege 15

username usuario03 password Usuario@123 max-sessions 1 privilege 15

Criando a rota IP para gerencia OUTBAND

ZXAN(config)# ip route 0.0.0.0 0.0.0.0 136.1.1.1

ZXAN(config)# no ssh server only

Configurando rack, shelf e as placas da OLT

ZXAN(config)# add-rack rackno 1 racktype C320Rack

ZXAN(config)# add-shelf shelfno 1 shelftype C320_SHELF

ZXAN(config)# set-pnp enable

ZXAN(config)# show card

Criando VLAN 1000 para gerencia IN-BAND

ZXAN(config)# vlan 1000

ZXAN(config-vlan)# description gerencia

ZXAN(config-vlan)# exit

Atribuindo IP à vlan 1000 de gerencia - Gerencia INBAND

ZXAN(config)# interface vlan 1000

ZXAN(config-if)# ip address 172.16.4.2 255.255.255.0

ZXAN(config-if)# exit

Criamos a rota para a gerencia Inband

ZXAN(config)# ip route 172.16.4.0 255.255.255.0 172.16.4.1

Vincular a vlan de gerencia na porta de uplink

ZXAN(config)# interface gei_1/4/1

ZXAN(config-if)# no shutdown

ZXAN(config-if)# switchport mode trunk

ZXAN(config-if)# switchport vlan 1000 tag

ZXAN(config-if)# exit

Ajustar fuso horario

ZXAN(config)# clock timezone GMT-3 -3 0

Ajustamos hora/data

ZXAN# clock set 18:29:00 aug 18 2021

Configurar o NTP

ZXAN(config)# ntp enable

ZXAN(config)# ntp server 200.189.40.8

Configurar o auto-write ou auto-save

ZXAN(config)# auto-write enable

ZXAN(config)# auto-write 03:00:00 everyday

Configurar o auto-backup

ZXAN(config)# file-server auto-backup cfg server-index 1 ipaddress 136.1.1.15 ftp user user01 password user01

ZXAN(config)# vlan 12

ZXAN(config-vlan)# description iptv

ZXAN(config-vlan)# exit

Vincular as vlans de servoço na porta de uplink

ZXAN(config)# interface gei_1/4/3

ZXAN(config-if)# switchport vlan 10-12 tag

ZXAN(config-if)# exit

ZXAN(config-if)# show vlan port gei_1/4/3

Configurando o pefil GPON ONU VLAN para vlans 10 11 e 12

ZXAN(config)# gpon

ZXAN(config-gpon)# onu profile vlan vlan-10 tag-mode tag cvlan 10

ZXAN(config-gpon)# onu profile vlan vlan-11 tag-mode tag cvlan 11

ZXAN(config-gpon)# onu profile vlan vlan-12 tag-mode tag cvlan 12

ZXAN(config-gpon)# onu profile vlan vlan-20 tag-mode tag cvlan 20

ZXAN(config-gpon)# exit

ZXAN(config)# show gpon onu profile vlan

Configurando o PROFILE T-CONT

ZXAN(config)# gpon

ZXAN(config-gpon)# profile tcont 100m type 4 maximum 105000

ZXAN(config-gpon)# profile tcont 1g type 4 maximum 1000000

ZXAN(config)# show gpon profile tcont

Criando template de ONU TYPE: ZTE-F660V5.2 com 4FE,2POTS

show onu-type gpon

ZXAN(config)# pon

ZXAN(config-pon)# onu-type ZTE-F660 gpon description 4FE,1POTS

ZXAN(config-pon)# onu-type ZTE-F660 gpon max-tcont 8

ZXAN(config-pon)# onu-type ZTE-F660 gpon max-gemport 255

ZXAN(config-pon)# onu-type ZTE-F660 gpon max-switch-perslot 8

ZXAN(config-pon)# onu-type ZTE-F660 gpon max-flow-perswitch 32

ZXAN(config-pon)# onu-type ZTE-F660 gpon max-iphost 10

ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/1

ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/2

ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/3

ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/4

ZXAN(config-pon)# onu-type-if ZTE-F660 pots_0/1

ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/1

ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/2

ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/3

ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/4

Habilitando a porta GPON

ZXAN(config)# interface gpon-olt_1/2/1

ZXAN(config-if)# no shutdown

ZXAN(config-if)# exit

ZXAN(config)# interface gpon-olt_1/2/2

ZXAN(config-if)# no shutdown

ZXAN(config-if)# exit

ZXAN(config)# interface gpon-olt_1/2/3

ZXAN(config-if)# no shutdown

ZXAN(config-if)# exit

Encontrar a ONU que queremos provisionar

ZXAN(config)# show gpon onu uncfg

Index Sn State

---------------------------------------------------------------------

gpon-onu_1/2/1:1 ZTEGC4B04358 unknown

gpon-onu_1/2/1:2 ZTEGC4B05AC0 unknown

gpon-onu_1/2/2:1 ZTEGC4B062CD unknown

gpon-onu_1/2/2:2 ZTEGC4B05A90 unknown

Adicionar a ONU na porta PON

ZXAN(config)# interface gpon-olt_1/2/1

ZXAN(config-if)# onu 1 type ZTE-F601 sn ZTEGC4B04358 .

[Successful]

ZXAN(config-if)# show gpon onu state

OnuIndex Admin State OMCC State O7 State Phase State

----------------------------------------------------------------------------

gpon-onu_1/2/1:1 enable enable operation working

ZXAN(config-if)# exit

Configurar o tunel GPON da ONU

ZXAN(config)# interface gpon-onu_1/2/1:1

ZXAN(config-if)# tcont 1 profile 100m

ZXAN(config-if)# gemport 1 tcont 1

CVLAN: 10

CVLAN priority: 0

SVLAN: 0

Current IP: 10.10.10.200

Current mask: 255.255.255.255

Current gateway:10.10.10.100

Current primary DNS: 8.8.8.8

Current secondary DNS: 0.0.0.0

Domain name:

Host name: omci_ipv4_pppoe_1

MAC address: e019.54c4.019b

IP host id: 1

ZXAN(config)# show gpon onu detail-info gpon-onu_1/2/2:1

ZXAN(config)# show pon power onu-rx gpon-olt_1/2/2

ZXAN(config)# show pon power onu-rx gpon-onu_1/2/2:1

=================================================================================== =

============== SCRIPT DE PROVISIONAMENTO DE ONU NA C300 =========================== ===================================================================================

PPPoE/DHCP/IP

interface gpon-olt_1/2/1

no onu 1

exit

interface gpon-olt_1/2/1

onu 1 type ZTE-F601 sn ZTEGC4B062CD

exit

interface gpon-onu_1/2/1:1 name teste-dupla

tcont 1 profile 100m gemport 1 name internet unicast tcont 1

service-port 1 vport 1 user-vlan 10 vlan 10

exit

pon-onu-mng gpon-onu_1/2/1:1

service 1 gemport 1 vlan 10

exit

BRIDGE

pon-onu-mng gpon-onu_1/2/1:1

vlan port eth_0/1 mode tag vlan 10

exit

show gpon onu baseinfo gpon-olt_1/2/2

show gpon remote-onu wan-ip gpon-onu_1/2/1:1

SSID de 5 a 8 para 5Ghz

pon-onu-mng gpon-onu_1/2/2:3

service 1 gemport 1 vlan 600

wan-ip 1 mode pppoe username nome password *** vlan-profile 600PPPOE host 1

wan-ip 1 ping-response enable traceroute-response enable security-mgmt 1 state enable

mode forward ingress-type iphost 1 protocol web

wifi enable channel 6

ssid auth wpa wifi_0/1 key 10203040

ssid auth wpa wifi_0/4 key 10203040

ssid ctrl wifi_0/1 name foton2154-2G

ssid ctrl wifi_0/4 name foton2154-5G

Mostrar valores de conexão

ZXAN(config)# show pon power onu-rx gpon-onu_1/2/1:1

Onu Rx power

------------------------------------

gpon-onu_1/2/1:1 -15.751(dbm)

ZXAN(config)# show pon power onu-rx gpon-olt_1/2/1

ZXAN(config)# show pon power attenuation gpon-onu_1/2/1:1

0
Tags:
Created by Jean Franco on 2024/06/09 12:45

- Comments (0)
- Attachments (0)
- History
- Information

# Applications

# Tips

Did you know that you can improve XWiki? Take 5 minutes to fill this survey and help this open source project!

Maila Networks
XWiki Debian 14.4.1