# Wiki source code of Comissionamento

Last modified by Jean Franco on 2024/06/10 17:56
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Show last authors

author | version | line-number | content
--- | --- | --- | ---
|  | 1 | **Criando usuários:**
|  | 2 |
|  | 3 | username zte password zte max-sessions 1 privilege 15
|  | 4 |
|  | 5 | username usuario01 password Usuario@123 max-sessions 1 privilege 15
|  | 6 |
|  | 7 | username usuario02 password Usuario@123 max-sessions 1 privilege 15
|  | 8 |
|  | 9 | username usuario03 password Usuario@123 max-sessions 1 privilege 15
|  | 10 |
|  | 11 | **Criando a rota IP para gerencia OUTBAND**
|  | 12 |
|  | 13 | ZXAN(config)# ip route 0.0.0.0 0.0.0.0 136.1.1.1
|  | 14 |
|  | 15 | ZXAN(config)# no ssh server only
|  | 16 |
|  | 17 | **Configurando rack, shelf e as placas da OLT**
|  | 18 |
|  | 19 | ZXAN(config)# add-rack rackno 1 racktype C320Rack
|  | 20 |
|  | 21 | ZXAN(config)# add-shelf shelfno 1 shelftype C320_SHELF
|  | 22 |
|  | 23 | ZXAN(config)# set-pnp enable
|  | 24 |
|  | 25 | ZXAN(config)# show card
|  | 26 |
|  | 27 | **Criando VLAN 1000 para gerencia IN-BAND**
|  | 28 |
|  | 29 | ZXAN(config)# vlan 1000
|  | 30 |
|  | 31 | ZXAN(config-vlan)# description gerencia
|  | 32 |
|  | 33 | ZXAN(config-vlan)# exit
|  | 34 |
|  | 35 | **Atribuindo IP à vlan 1000 de gerencia - Gerencia INBAND**
|  | 36 |
|  | 37 | ZXAN(config)# interface vlan 1000
|  | 38 |
|  | 39 | ZXAN(config-if)# ip address 172.16.4.2 255.255.255.0
|  | 40 |
|  | 41 | ZXAN(config-if)# exit
|  | 42 |
|  | 43 | **Criamos a rota para a gerencia Inband**
|  | 44 |
|  | 45 | ZXAN(config)# ip route 172.16.4.0 255.255.255.0 172.16.4.1
|  | 46 |
|  | 47 | Vincular a vlan de gerencia na porta de uplink
|  | 48 |
|  | 49 | ZXAN(config)# interface gei_1/4/1
|  | 50 |
|  | 51 | ZXAN(config-if)# no shutdown
|  | 52 |
|  | 53 | ZXAN(config-if)# switchport mode trunk
|  | 54 |
|  | 55 | ZXAN(config-if)# switchport vlan 1000 tag
|  | 56 |
|  | 57 | ZXAN(config-if)# exit
|  | 58 |
|  | 59 |
|  | 60 | **Ajustar fuso horario**
|  | 61 |
|  | 62 | ZXAN(config)# clock timezone GMT-3 -3 0
|  | 63 |
|  | 64 |
|  | 65 | **Ajustamos hora/data**
|  | 66 |
|  | 67 | ZXAN# clock set 18:29:00 aug 18 2021
|  | 68 |
|  | 69 |
|  | 70 | **Configurar o NTP**
|  | 71 |
|  | 72 | ZXAN(config)# ntp enable
|  | 73 |
|  | 74 | ZXAN(config)# ntp server 200.189.40.8
|  | 75 |
|  | 76 | **Configurar o auto-write ou auto-save**
|  | 77 |
|  | 78 | ZXAN(config)# auto-write enable
|  | 79 |
|  | 80 | ZXAN(config)# auto-write 03:00:00 everyday
|  | 81 |
|  | 82 |
|  | 83 | **Configurar o auto-backup**
|  | 84 |
|  | 85 | ZXAN(config)# file-server auto-backup cfg server-index 1 ipaddress 136.1.1.15 ftp user user01 password user01
|  | 86 |
|  | 87 |
|  | 88 |
|  | 89 | ZXAN(config)# vlan 12
|  | 90 |
|  | 91 | ZXAN(config-vlan)# description iptv
|  | 92 |
|  | 93 | ZXAN(config-vlan)# exit
|  | 94 |
|  | 95 |
|  | 96 | **Vincular as vlans de servoço na porta de uplink**
|  | 97 |
|  | 98 | ZXAN(config)# interface gei_1/4/3
|  | 99 |
|  | 100 | ZXAN(config-if)# switchport vlan 10-12 tag
|  | 101 |
|  | 102 | ZXAN(config-if)# exit
|  | 103 |
|  | 104 | ZXAN(config-if)# show vlan port gei_1/4/3
|  | 105 |
|  | 106 |
|  | 107 | **Configurando o pefil GPON ONU VLAN para vlans 10 11 e 12**
|  | 108 |
|  | 109 | ZXAN(config)# gpon
|  | 110 |
|  | 111 | ZXAN(config-gpon)# onu profile vlan vlan-10 tag-mode tag cvlan 10
|  | 112 |
|  | 113 | ZXAN(config-gpon)# onu profile vlan vlan-11 tag-mode tag cvlan 11
|  | 114 |
|  | 115 | ZXAN(config-gpon)# onu profile vlan vlan-12 tag-mode tag cvlan 12
|  | 116 |
|  | 117 | ZXAN(config-gpon)# onu profile vlan vlan-20 tag-mode tag cvlan 20
|  | 118 |
|  | 119 | ZXAN(config-gpon)# exit
|  | 120 |
|  | 121 | ZXAN(config)# show gpon onu profile vlan
|  | 122 |
|  | 123 |
|  | 124 | **Configurando o PROFILE T-CONT**
|  | 125 |
|  | 126 | ZXAN(config)# gpon
|  | 127 |
|  | 128 | ZXAN(config-gpon)# profile tcont 100m type 4 maximum 105000
|  | 129 |
|  | 130 | ZXAN(config-gpon)# profile tcont 1g type 4 maximum 1000000
|  | 131 |
|  | 132 | ZXAN(config)# show gpon profile tcont
|  | 133 |
|  | 134 |
|  | 135 | **Criando template de ONU TYPE: ZTE-F660V5.2 com 4FE,2POTS**
|  | 136 |
|  | 137 | show onu-type gpon
|  | 138 |
|  | 139 | ZXAN(config)# pon
|  | 140 |
|  | 141 | ZXAN(config-pon)# onu-type ZTE-F660 gpon description 4FE,1POTS
|  | 142 |
|  | 143 | ZXAN(config-pon)# onu-type ZTE-F660 gpon max-tcont 8
|  | 144 |
|  | 145 | ZXAN(config-pon)# onu-type ZTE-F660 gpon max-gemport 255
|  | 146 |
|  | 147 | ZXAN(config-pon)# onu-type ZTE-F660 gpon max-switch-perslot 8
|  | 148 |
|  | 149 | ZXAN(config-pon)# onu-type ZTE-F660 gpon max-flow-perswitch 32
|  | 150 |
|  | 151 | ZXAN(config-pon)# onu-type ZTE-F660 gpon max-iphost 10
|  | 152 |
|  | 153 | ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/1
|  | 154 |
|  | 155 | ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/2
|  | 156 |
|  | 157 | ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/3
|  | 158 |
|  | 159 | ZXAN(config-pon)# onu-type-if ZTE-F660 eth_0/4
|  | 160 |
|  | 161 | ZXAN(config-pon)# onu-type-if ZTE-F660 pots_0/1
|  | 162 |
|  | 163 | ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/1
|  | 164 |
|  | 165 | ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/2
|  | 166 |
|  | 167 | ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/3
|  | 168 |
|  | 169 | ZXAN(config-pon)# onu-type-if ZTE-F660 wifi_0/4
|  | 170 |
|  | 171 | **Habilitando a porta GPON**
|  | 172 |
|  | 173 | ZXAN(config)# interface gpon-olt_1/2/1
|  | 174 |
|  | 175 | ZXAN(config-if)# no shutdown
|  | 176 |
|  | 177 | ZXAN(config-if)# exit
|  | 178 |
|  | 179 | ZXAN(config)# interface gpon-olt_1/2/2
|  | 180 |
|  | 181 | ZXAN(config-if)# no shutdown
|  | 182 |
|  | 183 | ZXAN(config-if)# exit
|  | 184 |
|  | 185 | ZXAN(config)# interface gpon-olt_1/2/3
|  | 186 |
|  | 187 | ZXAN(config-if)# no shutdown
|  | 188 |
|  | 189 | ZXAN(config-if)# exit
|  | 190 |
|  | 191 |
|  | 192 | **Encontrar a ONU que queremos provisionar**
|  | 193 |
|  | 194 | ZXAN(config)# show gpon onu uncfg
|  | 195 |
|  | 196 | Index Sn State
|  | 197 |
|  | 198 | ~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~--
|  | 199 |
|  | 200 | gpon-onu_1/2/1:1 ZTEGC4B04358 unknown
|  | 201 |
|  | 202 | gpon-onu_1/2/1:2 ZTEGC4B05AC0 unknown
|  | 203 |
|  | 204 | gpon-onu_1/2/2:1 ZTEGC4B062CD unknown
|  | 205 |
|  | 206 | gpon-onu_1/2/2:2 ZTEGC4B05A90 unknown
|  | 207 |
|  | 208 |
|  | 209 | **Adicionar a ONU na porta PON**
|  | 210 |
|  | 211 | ZXAN(config)# interface gpon-olt_1/2/1
|  | 212 |
|  | 213 | ZXAN(config-if)# onu 1 type ZTE-F601 sn ZTEGC4B04358 .
|  | 214 |
|  | 215 | [Successful]
|  | 216 |
|  | 217 |
|  | 218 | ZXAN(config-if)# show gpon onu state
|  | 219 |
|  | 220 | OnuIndex Admin State OMCC State O7 State Phase State
|  | 221 |
|  | 222 | ~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-
|  | 223 |
|  | 224 | gpon-onu_1/2/1:1 enable enable operation working
|  | 225 |
|  | 226 | ZXAN(config-if)# exit
|  | 227 |
|  | 228 |
|  | 229 | **Configurar o tunel GPON da ONU**
|  | 230 |
|  | 231 | ZXAN(config)# interface gpon-onu_1/2/1:1
|  | 232 |
|  | 233 | ZXAN(config-if)# tcont 1 profile 100m
|  | 234 |
|  | 235 | ZXAN(config-if)# gemport 1 tcont 1
|  | 236 |
|  | 237 |
|  | 238 |
|  | 239 |
|  | 240 | CVLAN: 10
|  | 241 |
|  | 242 | CVLAN priority: 0
|  | 243 |
|  | 244 | SVLAN: 0
|  | 245 |
|  | 246 | Current IP: 10.10.10.200
|  | 247 |
|  | 248 | Current mask: 255.255.255.255
|  | 249 |
|  | 250 | Current gateway:10.10.10.100
|  | 251 |
|  | 252 | Current primary DNS: 8.8.8.8
|  | 253 |
|  | 254 | Current secondary DNS: 0.0.0.0
|  | 255 |
|  | 256 | Domain name:
|  | 257 |
|  | 258 | Host name: omci_ipv4_pppoe_1
|  | 259 |
|  | 260 | MAC address: e019.54c4.019b
|  | 261 |
|  | 262 | IP host id: 1
|  | 263 |
|  | 264 | ZXAN(config)# show gpon onu detail-info gpon-onu_1/2/2:1
|  | 265 |
|  | 266 | ZXAN(config)# show pon power onu-rx gpon-olt_1/2/2
|  | 267 |
|  | 268 | ZXAN(config)# show pon power onu-rx gpon-onu_1/2/2:1
|  | 269 |
|  | 270 |
|  | 271 | ~=================================================================================== =
|  | 272 |
|  | 273 | ~============== SCRIPT DE PROVISIONAMENTO DE ONU NA C300 =========================== ===================================================================================
|  | 274 |
|  | 275 | **PPPoE/DHCP/IP**
|  | 276 |
|  | 277 | interface gpon-olt_1/2/1
|  | 278 |
|  | 279 | no onu 1
|  | 280 |
|  | 281 | exit
|  | 282 |
|  | 283 | interface gpon-olt_1/2/1
|  | 284 |
|  | 285 | onu 1 type ZTE-F601 sn ZTEGC4B062CD
|  | 286 |
|  | 287 | exit
|  | 288 |
|  | 289 | interface gpon-onu_1/2/1:1 name teste-dupla
|  | 290 |
|  | 291 | tcont 1 profile 100m gemport 1 name internet unicast tcont 1
|  | 292 |
|  | 293 | service-port 1 vport 1 user-vlan 10 vlan 10
|  | 294 |
|  | 295 | exit
|  | 296 |
|  | 297 | pon-onu-mng gpon-onu_1/2/1:1
|  | 298 |
|  | 299 | service 1 gemport 1 vlan 10
|  | 300 |
|  | 301 | exit
|  | 302 |
|  | 303 |
|  | 304 | **BRIDGE**
|  | 305 |
|  | 306 | pon-onu-mng gpon-onu_1/2/1:1
|  | 307 |
|  | 308 | vlan port eth_0/1 mode tag vlan 10
|  | 309 |
|  | 310 | exit
|  | 311 |
|  | 312 |
|  | 313 | show gpon onu baseinfo gpon-olt_1/2/2
|  | 314 |
|  | 315 | show gpon remote-onu wan-ip gpon-onu_1/2/1:1
|  | 316 |
|  | 317 |
|  | 318 | SSID de 5 a 8 para 5Ghz
|  | 319 |
|  | 320 | pon-onu-mng gpon-onu_1/2/2:3
|  | 321 |
|  | 322 | service 1 gemport 1 vlan 600
|  | 323 |
|  | 324 | wan-ip 1 mode pppoe username nome password ~*~** vlan-profile 600PPPOE host 1
|  | 325 |
|  | 326 | wan-ip 1 ping-response enable traceroute-response enable security-mgmt 1 state enable
|  | 327 |
|  | 328 | mode forward ingress-type iphost 1 protocol web
|  | 329 |
|  | 330 | wifi enable channel 6
|  | 331 |
|  | 332 | ssid auth wpa wifi_0/1 key 10203040
|  | 333 |
|  | 334 | ssid auth wpa wifi_0/4 key 10203040
|  | 335 |
|  | 336 | ssid ctrl wifi_0/1 name foton2154-2G
|  | 337 |
|  | 338 | ssid ctrl wifi_0/4 name foton2154-5G
|  | 339 |
|  | 340 |
|  | 341 | **Mostrar valores de conexão**
|  | 342 |
|  | 343 | ZXAN(config)# show pon power onu-rx gpon-onu_1/2/1:1
|  | 344 |
|  | 345 | Onu Rx power
|  | 346 |
|  | 347 | ~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-~-
|  | 348 |
|  | 349 | gpon-onu_1/2/1:1 -15.751(dbm)
|  | 350 |
|  | 351 |
|  | 352 | ZXAN(config)# show pon power onu-rx gpon-olt_1/2/1
|  | 353 |
|  | 354 |
|  | 355 | ZXAN(config)# show pon power attenuation gpon-onu_1/2/1:1
|  | 356 |
|  | 357 |

# Applications

# Tips

Jump to any page in the wiki with Ctrl+G or Meta+G.
See more shortcuts.

Maila Networks
XWiki Debian 14.4.1