# Wiki source code of Script de provisionamento

Last modified by Jean Franco on 2024/06/09 15:32
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Show last authors

author | version | line-number | content
--- | --- | --- | ---
|  | 1 | Script de provisionamento:
|  | 2 |
|  | 3 | interface gpon-olt_#pon_id#
|  | 4 | onu #onu_numero# type ZTE-F660 sn #onu_mac#
|  | 5 | onu #onu_numero# profile line padrao01
|  | 6 | exit
|  | 7 | interface gpon-onu_#pon_id#:#onu_numero#
|  | 8 | service-port 1 vport 1 user-vlan #vlan# vlan #vlan#
|  | 9 | exit
|  | 10 | pon-onu-mng gpon-onu_#pon_id#:#onu_numero#
|  | 11 | service INTERNET gemport 1 vlan #vlan#
|  | 12 | wan-ip 1 mode pppoe username #pppoe_login# password #pppoe_senha# vlan-profile INT-#vlan# host 1
|  | 13 | pppoe 1 nat enable user #pppoe_login# password #pppoe_senha#;security-mgmt 1 state enable mode forward ingress-type wan protocol web
|  | 14 |
|  | 15 |
|  | 16 | Provisionando ONU em Bridge - 1 porta:
|  | 17 |
|  | 18 | interface gpon-olt_#pon_id#; onu #onu_numero# type ZTE-F600 sn #onu_mac#; onu #onu_numero# profile PROFILE-ONU; exit; interface gpon-onu_#pon_id#:#onu_numero#; service-port 1 vport 1 user-vlan #vlan# vlan #vlan#;exit; pon-onu-mng gpon-onu_#pon_id#:#onu_numero#; service INTERNET-SERVICE gemport 1 vlan #vlan#; vlan port eth_0/1 mode tag vlan #vlan#;
|  | 19 |
|  | 20 | Provisionando ONU em Bridge - 4 portas:
|  | 21 |
|  | 22 | interface gpon-olt_#pon_id#; onu #onu_numero# type ZTE-F600 sn #onu_mac#; onu #onu_numero# profile PROFILE-ONU; exit; interface gpon-onu_#pon_id#:#onu_numero#; service-port 1 vport 1 user-vlan #vlan# vlan #vlan#;exit; pon-onu-mng gpon-onu_#pon_id#:#onu_numero#; service INTERNET-SERVICE gemport 1 vlan #vlan#; vlan port eth_0/1 mode tag vlan #vlan#; vlan port eth_0/2 mode tag vlan #vlan#; vlan port eth_0/3 mode tag vlan #vlan#; vlan port eth_0/4 mode tag vlan #vlan#;
|  | 23 |
|  | 24 | Provisionando em modo roteador com PPPoE:
|  | 25 |
|  | 26 | interface gpon-olt_#pon_id#; onu #onu_numero# type ZTE-F600 sn #onu_mac#; onu #onu_numero# profile PROFILE-ONU; exit; interface gpon-onu_#pon_id#:#onu_numero#; service-port 1 vport 1 user-vlan #vlan# vlan #vlan#; exit; pon-onu-mng gpon-onu_#pon_id#:#onu_numero#; service INTERNET-SERVICE gemport 1 iphost 1 vlan #vlan#; wan-ip 1 mode pppoe username #pppoe_login# password #pppoe_senha# vlan-profile PROFILE-PPPOE host 1; pppoe 1 nat enable user #pppoe_login# password #pppoe_senha#; security-mgmt 1 state enable mode forward ingress-type iphost 1 protocol web;
|  | 27 |
|  | 28 |
|  | 29 |

# Applications

# Tips

Jump to any page in the wiki with Ctrl+G or Meta+G.
See more shortcuts.

Maila Networks
XWiki Debian 14.4.1