# Wiki source code of Instalando o SysrescueCD num pendrive

Last modified by Jean Franco on 2022/06/27 20:43
Export
Office Formats
Export as PDF Export as ODT Export as RTF
Other Formats

Select the pages to export:

select all/ none

Legend:
  Created Page
  Modified Extension Page
  Clean Extension Page

Export as HTML

Show last authors

author | version | line-number | content
--- | --- | --- | ---
|  | 1 | Steps for installing system rescue CD on USB are mentioned on [[http:~~/~~/www.sysresccd.org/Sysresccd-manual-en_How_to_install_SystemRescueCd_on_an_USB-stick>>url:http://www.sysresccd.org/Sysresccd-manual-en_How_to_install_SystemRescueCd_on_an_USB-stick]]. Automated steps to install from linux using shell script do not work. Detailed steps that work are:
|  | 2 |
|  | 3 | * Create folder for USB - '##mkdir /mnt/usbstick##'
|  | 4 | * Mount USB (Fat32) partition: '##mount -t vfat /dev/sdf1 /mnt/usbstick##'
|  | 5 | * Remove all files: '##rm -rf /mnt/usbstick/*##'
|  | 6 | * Download latest system rescue CD image and mount it on ##/mnt/cdrom## using '##mount -o loop <iso_file> /mnt/cdrom##'
|  | 7 | * Use following commands to copy files to USB
|  | 8 |
|  | 9 | {{{cp -af /mnt/cdrom/* /mnt/usbstick/
|  | 10 | rm -rf /mnt/usbstick/syslinux
|  | 11 | mv /mnt/usbstick/isolinux/isolinux.cfg /mnt/usbstick/isolinux/syslinux.cfg
|  | 12 | sed -i -e 's/scandelay=1/scandelay=5/g' /mnt/usbstick/isolinux/syslinux.cfg
|  | 13 | mv /mnt/usbstick/isolinux /mnt/usbstick/syslinux
|  | 14 | }}}
|  | 15 |
|  | 16 | * Make disk bootable using
|  | 17 |
|  | 18 | {{{umount /mnt/usbstick
|  | 19 | syslinux /dev/sdf1
|  | 20 | sync}}}

# Applications

# Tips

Press the x+x+x+a key combo to toggle the Advanced mode and x+x+x+h to toggle the display of hidden pages.

Maila Networks
XWiki Debian 14.4.1